L1 8-1/2” Reaming Run   
Mud Pits Plan

# Objective:

* Treat active system with shale inhibition and bridging material while reaming.
* Increase Mud active system volume to prepare Sealing pill (CSG go pill).
* Prepare Hi-Vis to sweep hole every 10 stands.

# Procedures:

* **While RIH from surface with reaming**
* **Increase Mud active system volume to prepare Sealing pill (CSG go pill).**
  1. Transfer all barite free Rheliant OBM from Pit #7 to Pit #5
  2. Transfer all barite Rheliant OBM from Pit #3 to Pit #7
  3. Open Equalizer between pit #7 and pit #6
  4. Line up active pits as pit #7 Return and pit #6 Suction.
* **While Reaming down:**
* **Treat active system with shale inhibition and bridging material while reaming:**

Mix the following in active pit #7

* + One time only:
    - Marble Medium 🡺 1 Big Bag
  + Hourly treatment:
    - Poroseal 🡺 4 drum
    - Baracarb 50 🡺 1 sack
    - Baracarb 25 🡺 1 sack
    - Steal Seal SF 🡺 1 sack
* **Prepare Hi-Vis to sweep hole every 10 stands:**
  + In Slug #10: prepare Hi-Vis as needed:
  + Transfer 70 bbl from active pit to slug #10, then mix:
    - VG Plus 🡺 1 sack
    - VG Supreme 🡺 1 sack
* **At TD:**
* **Increase active system M-WT to 96 PCF by adding 10,000 lb Barite**
* **While POOH to window:**
* **prepare Sealing pill (CSG go pill).**
  1. Close Equalizer between pit #7 & pit #6:
  2. Keep Pit #6 as active pit, Suction and return.
  3. Maintain pit #7 volume 300 bbl.
  4. Mix the following in pit #7 as CSG go pill :
     + Baracarb 50 🡺 30 sack
     + Baracarb 25 🡺 30 sack
     + Steal Seal SF 🡺 30 sack
     + Marble Medium 🡺 1 Big Bag
     + Lubraglide 🡺 6 sacks

* 1. Transfer all barite free Rheliant OBM from Pit #7 to Pit #5
  2. Transfer all barite Rheliant OBM from Pit #3 to Pit #7
  3. Open Equalizer between pit #7 and pit #6
  4. Line up active pits as pit #7 Return and pit #6 Suction.

------------------------------------------------------------------------------------------------------

# Procedures: while RIH with reaming :

***Thanks and work SAFE***